{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":4,"rows_kept":35,"flags":["formulas_cached_only"]}
["IP","类型","KEY","描述"]
["192.168.170.61","质量中心","RunState","机器人状态"]
["192.168.170.61","质量中心","ExplorerState","三坐标状态"]
["192.168.170.61","质量中心","AGVState","AGV接驳位状态"]
["192.168.170.61","质量中心","MachineAlarm","PLC是否正常"]
[]
["192.168.170.71","柔性线","RunState","机器人状态"]
["192.168.170.71","柔性线","AGVState","AGV接驳位状态"]
["192.168.170.71","柔性线","CleanAlarm","清洗机是否故障"]
["192.168.170.71","柔性线","AllowPrint","是否允许打标"]
["192.168.170.71","柔性线","MachineAlarm","PLC是否正常"]
[]
["192.168.170.81","智能单元","RunState","机器人状态"]
["192.168.170.81","智能单元","AGVState","AGV接驳位状态"]
["192.168.170.81","智能单元","MachineAlarm","PLC是否正常"]
[]
["192.168.170.206","柔性线机床","MainProgNo","主程序号"]
["192.168.170.206","柔性线机床","CncSumBootTime","系统累计开机时间"]
["192.168.170.206","柔性线机床","CutRate","切削倍率"]
["192.168.170.206","柔性线机床","SpRate","主轴倍率"]
["192.168.170.206","柔性线机床","SpActSpeed","主轴实际速度"]
["192.168.170.206","柔性线机床","ProRunState","程序运行状态"]
["192.168.170.206","柔性线机床","AllowFetchMaterial","机床允许取料"]
["192.168.170.206","柔性线机床","AllowPutMaterial","机床允许放料"]
["192.168.170.206","柔性线机床","MachineAlarm","PLC是否正常"]
[]
["192.168.170.205","智能单元机床","MainProgNo","主程序号"]
["192.168.170.205","智能单元机床","CncSumBootTime","系统累计开机时间"]
["192.168.170.205","智能单元机床","CutRate","切削倍率"]
["192.168.170.205","智能单元机床","SpRate","主轴倍率"]
["192.168.170.205","智能单元机床","SpActSpeed","主轴实际速度"]
["192.168.170.205","智能单元机床","ProRunState","程序运行状态"]
["192.168.170.205","智能单元机床","AllowFetchMaterial","机床允许取料"]
["192.168.170.205","智能单元机床","AllowPutMaterial","机床允许放料"]
["192.168.170.205","智能单元机床","MachineAlarm","PLC是否正常"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}